{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA50A2VEB","ADEA100A2VEB"]
["Ventilador","Pressão estática disponível","","Alto","Pa","","150"]
["Envolvente","Cor","","","","","Não pintado (galvanizado)"]
["Envolvente","Material","","","","","Chapa de aço galvanizado"]
["Dimensões","Unidade","","Altura","mm","","245"]
["","","","Largura","mm","","1400"]
["","","","Profundidade","mm","","800"]
["Peso","Unidade","","","kg","","46"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","","29"]
["Ventilador","Caudal de ar","Arrefecimento","Medium","m³/min","","26"]
["Ventilador","Caudal de ar","Arrefecimento","B","m³/min","","23"]
["","","Aquecimento","Alto","m³/min","","29"]
["Ventilador","Caudal de ar","Aquecimento","Medium","m³/min","","26"]
["Ventilador","Caudal de ar","Aquecimento","B","m³/min","","23"]
["","Pressão estática disponível","","Nom.","Pa","","40"]
["Nível de potência sonora","Arrefecimento","","","dBA","","58"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","","34"]
["Nível de pressão sonora","Arrefecimento","","Medium","dBA","","32"]
["Nível de pressão sonora","Arrefecimento","","B","dBA","","30"]
["","Aquecimento","","Alto","dBA","","36"]
["","","","Médio","dBA","","33"]
["","","","B","dBA","","30"]
["Ligações de tubagem","Líquido","","DE","mm","","9.52"]
["Piping connections","Gás","","OD","mm","","15.9"]
["Ligações de tubagem","Esgoto","","","","","VP20 (I.D. 20/O.D. 26)"]
["Altura de drenagem","mm","","","","","625"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Acessórios standard","Installation manual","","","","","1"]
["","Washer for hanger bracket","","","","","8"]
["","Operation manual","","","","","1"]
["","Clamps","","","","","4"]
["","Drain hose","","","","","1"]
["","Insulation for fitting","","","","","2"]
["","Metal clamp for drain hose","","","","","1"]
["","Screws","","","","","40"]
["","Sealing pads","","","","","5"]
["Alimentação elétrica","Fase","","","","","1~"]
["Alimentação eléctrica","Alimentação eléctrica-=-Frequência","","Frequência","","","50"]
["","Alimentação eléctrica-=-Tensão","","Tensão","","","220-240/220"]
["Acessórios standard","AAA dry-cell batteries","","","","3"]