{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSRPS4A"]
[]
[]
[]
[]
["","","","","EKSRPS4A."]
["Instalação_","","","","Na lateral do depósito"]
["Dimensões","Unidade","Altura","mm","815"]
["","","Largura","mm","142"]
["","","Profundidade","mm","230"]
["Peso","Unidade","","kg","6"]
["Limite de funcionamento","Temperatura ambiente","Mín.","°C","5"]
["","","Máx.","°C","40"]
["Temperatura em inactividade","Máx.","","°C","85"]
["Controlo","Tipo","","","Controlador de diferença de temperatura digital com apresentação de texto plano"]
["Alimentação elétrica","Fase","","","1~"]
["Alimentação eléctrica","Alimentação eléctrica-=-Frequência","Frequência","","50"]
["","Alimentação eléctrica-=-Tensão","Tensão","","230"]
["Controlo","Controlo-=-Consumo de energia","Consumo de energia","","2"]
["Power supply intake","","","","Unidade interior"]