{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P1","EKSV26P1"]
["Instalação_","","","","Vertical","Vertical"]
["Dimensões","Unidade","Altura","mm","2000","2000"]
["","","Largura","mm","1006","1300"]
["","","Profundidade","mm","85","85"]
["Peso","Unidade","","kg","35","42"]
["Volume","l","","","1.3","1.7"]
["Superfície","Exterior","","m²","2.01","2.60"]
["","Abertura","","m²","1.800","2.360"]
["","Absorsor","","m²","1.80","2.36"]
["Revestimento","","","","Micro-termómetro (absorção máx. de 96%, emissão de cerca de 5% +/-2%)","Micro-termómetro (absorção máx. de 96%, emissão de cerca de 5% +/-2%)"]
["Absorsor","","","","Tubo de cobre em forma de harpa com placa de alumínio revestida altamente selectiva soldada a laser","Tubo de cobre em forma de harpa com placa de alumínio revestida altamente selectiva soldada a laser"]
["Vidro","","","","Vidro de segurança de painel único, transmissão +/- 92%","Vidro de segurança de painel único, transmissão +/- 92%"]
["Ângulo de telhado permitido","Mín.","","°","15","15"]
["","Máx.","","°","80","80"]
["Pressão de funcionamento","Máx.","","bar","6","6"]
["Temperatura em inactividade","Máx.","","°C","192","192"]
["Desempenho térmico","Coeficiente de perda de calor a2","","W/m².K","4.300","4.300"]
["","Dependência da temperatura do coeficiente de perda de calor a2","","W/m².K²","0.006","0.006"]
["","Capacidade térmica","","kJ/K","4.9","6.5"]