{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ50MV1BS"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","","47"]
["","","","Médio","dBA","","41"]
["","","","Funcionamento silencioso","dBA","","25"]
["","","","B","dBA","","35"]
["","Arrefecimento","","Medium","dBA","","40"]
["","","","Funcionamento silencioso","dBA","","25"]
["","","","B","dBA","","35"]
["","","","Alto","dBA","","46"]
["Acessórios standard","Manual de funcionamento","","","","","1"]
["","Manual de instalação","","","","","1"]
["","Controle remoto sem fios","","","","","1"]
["","Pilhas secas AAA","","","","","2"]
["","Suporte do controle remoto","","","","","1"]
["","Parafusos de fixação para chapa de montagem","","","","","5"]
["","Chapa de montagem","","","","","1"]
["","Filtro desodorizante de apatite de titânio","","","","","2"]
["","Parafuso de fixação para suporte do controlo remoto","","","","","2"]
["","Parafusos de fixação da unidade interior","","","","","2"]
["","Tampa do parafuso","","","","","2"]
["","Kit adaptador WLAN","","","","","1"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","","ARC466A9"]
["Piping connections","Liquid","","OD","mm","","6.35"]
["","Gás","","OD","mm","","12.70"]
["","Drain","","","","","18"]
["Power input","Arrefecimento","","Nom.","kW","","0.033"]
["","Aquecimento","","Nom.","kW","","0.043"]
["Nível de potência sonora","Arrefecimento","","","dBA","","60"]
["","Aquecimento","","","dBA","","60"]
["Dimensões","Unidade","","Width","mm","","998"]
["","","","Depth","mm","","212"]
["","","","Altura","mm","","303"]
["Envolvente","Cor","","","","","Prateado"]
["Peso","Unidade","","","kg","","12"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","","12.6"]
["","","","Medium","m³/min","","10.5"]
["","","","B","m³/min","","8.1"]
["","","","Funcionamento silencioso","m³/min","","5.0"]
["","","Arrefecimento","B","m³/min","","6.8"]
["","","","Medium","m³/min","","8.9"]
["","","","Alto","m³/min","","10.9"]
["","","","Funcionamento silencioso","m³/min","","3.6"]
["Power supply","Fase","","","","","1~"]
["","Nome","","","","","V1"]
["","Frequência","","","Hz","","50"]
["","Tensão","","","V","","220-240"]
["Notas","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.023"]
["","Aquecimento","","Nom.","kW","0.031"]
["Envolvente","Cor","","","","Prateado"]
["Dimensões","Unidade","","Altura","mm","303"]
["","","","Largura","mm","998"]
["","","","Profundidade","mm","212"]
["Peso","Unidade","","","kg","12"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","8.9"]
["","","","Médio","m³/min","6.6"]
["","","","B","m³/min","4.4"]
["","","","Funcionamento silencioso","m³/min","2.6"]
["","","Aquecimento","Alto","m³/min","10.2"]
["","","","Médio","m³/min","8.4"]
["","","","B","m³/min","6.3"]
["","","","Funcionamento silencioso","m³/min","3.8"]
["Nível de potência sonora","Arrefecimento","","","dBA","54"]
["","Aquecimento","","","dBA","56"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","38"]
["","","","Médio","dBA","32"]
["","","","B","dBA","25"]
["","","","Funcionamento silencioso","dBA","19"]
["","Aquecimento","","Alto","dBA","40"]
["","","","Médio","dBA","34"]
["","","","B","dBA","28"]
["","","","Funcionamento silencioso","dBA","19"]
["Ligações de tubagem","Líquido","","DE","mm","6.35"]
["","Gás","","DE","mm","9.50"]
["","Esgoto","","","","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A9"]
["Acessórios standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","Fixing screw for remote controller holder","","","","2"]
["","WLAN adapter kit","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Fixing screws for mounting plate","","","","5"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Alimentação elétrica","Nome","","","","V1"]
["","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50"]
["","Tensão","","","V","220-240"]