{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BW","FTXJ25MV1BW","FTXJ35MV1BW","FTXJ50MV1BW"]
["Nível de pressão sonora","Aquecimento","","Alto","dBA","40","41","45","47"]
["","","","Médio","dBA","34","34","37","41"]
["","","","Funcionamento silencioso","dBA","19","19","20","25"]
["","","","B","dBA","28","28","29","35"]
["","Arrefecimento","","Medium","dBA","32","32","34","40"]
["","","","Funcionamento silencioso","dBA","19","19","20","25"]
["","","","B","dBA","25","25","26","35"]
["","","","Alto","dBA","38","38","45","46"]
["Acessórios standard","Manual de funcionamento","","","","1","1","1","1"]
["","Manual de instalação","","","","1","1","1","1"]
["","Controle remoto sem fios","","","","1","1","1","1"]
["","Pilhas secas AAA","","","","2","2","2","2"]
["","Suporte do controle remoto","","","","1","1","1","1"]
["","Parafusos de fixação para chapa de montagem","","","","5","5","5","5"]
["","Chapa de montagem","","","","1","1","1","1"]
["","Filtro desodorizante de apatite de titânio","","","","2","2","2","2"]
["","Parafuso de fixação para suporte do controlo remoto","","","","2","2","2","2"]
["","Parafusos de fixação da unidade interior","","","","2","2","2","2"]
["","Tampa do parafuso","","","","2","2","2","2"]
["","Kit adaptador WLAN","","","","1","1","1","1"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gás","","OD","mm","9.50","9.50","9.50","12.70"]
["","Drain","","","","18","18","18","18"]
["Power input","Arrefecimento","","Nom.","kW","0.023","0.023","0.033","0.033"]
["","Aquecimento","","Nom.","kW","0.031","0.033","0.042","0.043"]
["Nível de potência sonora","Arrefecimento","","","dBA","54","54","59","60"]
["","Aquecimento","","","dBA","56","56","59","60"]
["Dimensões","Unidade","","Width","mm","998","998","998","998"]
["","","","Depth","mm","212","212","212","212"]
["","","","Altura","mm","303","303","303","303"]
["Envolvente","Cor","","","","Branco","Branco","Branco","Branco"]
["Peso","Unidade","","","kg","12","12","12","12"]
["Ventilador","Caudal de ar","Aquecimento","Alto","m³/min","10.2","11.0","12.4","12.6"]
["","","","Medium","m³/min","8.4","8.6","9.6","10.5"]
["","","","B","m³/min","6.3","6.3","6.9","8.1"]
["","","","Funcionamento silencioso","m³/min","3.8","3.8","4.1","5.0"]
["","","Arrefecimento","B","m³/min","4.4","4.4","4.8","6.8"]
["","","","Medium","m³/min","6.6","6.6","7.8","8.9"]
["","","","Alto","m³/min","8.9","8.9","10.9","10.9"]
["","","","Funcionamento silencioso","m³/min","2.6","2.6","2.9","3.6"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Nome","","","","V1","V1","V1","V1"]
["","Frequência","","","Hz","50","50","50","50"]
["","Tensão","","","V","220-240","220-240","220-240","220-240"]
["Notas","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]