{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM42M2V1B"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.035"]
["","Aquecimento","","Nom.","kW","0.035"]
["Envolvente","Cor","","","","Branco"]
["Dimensões","Unidade","","Altura","mm","294"]
["","","","Largura","mm","811"]
["","","","Profundidade","mm","272"]
["Peso","Unidade","","","kg","10"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","12.6"]
["Ventilador","Caudal de ar","Arrefecimento","Medium","m³/min","9.5"]
["Ventilador","Caudal de ar","Arrefecimento","B","m³/min","7.1"]
["","","","Funcionamento silencioso","m³/min","4.6"]
["","","Aquecimento","Alto","m³/min","13"]
["Ventilador","Caudal de ar","Aquecimento","Medium","m³/min","10.4"]
["Ventilador","Caudal de ar","Aquecimento","B","m³/min","7.1"]
["","","","Funcionamento silencioso","m³/min","5.3"]
["Nível de potência sonora","Arrefecimento","","","dBA","60"]
["","Aquecimento","","","dBA","60"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","45"]
["Nível de pressão sonora","Arrefecimento","","Medium","dBA","39"]
["Nível de pressão sonora","Arrefecimento","","B","dBA","30"]
["","","","Funcionamento silencioso","dBA","21"]
["","Aquecimento","","Alto","dBA","45"]
["","","","Médio","dBA","39"]
["","","","B","dBA","29"]
["","","","Funcionamento silencioso","dBA","21"]
["Ligações de tubagem","Líquido","","DE","mm","6.35"]
["Piping connections","Gás","","OD","mm","12.7"]
["Ligações de tubagem","Esgoto","","","","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Acessórios standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Alimentação elétrica","Nome","","","","V1"]
["","Fase","","","","1~"]
["Alimentação eléctrica","Alimentação eléctrica-=-Frequência","","Frequência","","50"]
["","Alimentação eléctrica-=-Tensão","","Tensão","","220-240"]