{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG35K2V1B"]
["Potência nominal","Arrefecimento","","Nom.","kW","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)"]
["","Aquecimento","","Nom.","kW","0.024 (1) (2) (3), 0.024 (1) (2) (3), 0.024 (1) (2) (3)"]
["Envolvente","Cor","","","","Branco fresco (6.5Y 9.5/0.5)"]
["Dimensões","Unidade","","Altura","mm","600"]
["","","","Largura","mm","950"]
["","","","Profundidade","mm","215"]
["Peso","Unidade","","","kg","22.0"]
["Ventilador","Caudal de ar","Arrefecimento","Alto","m³/min","9.1"]
["","","","Médio","m³/min","7.2"]
["","","","B","m³/min","5.3"]
["","","","Funcionamento silencioso","m³/min","4.5"]
["","","Aquecimento","Alto","m³/min","10.2"]
["","","","Médio","m³/min","8.0"]
["","","","B","m³/min","5.8"]
["","","","Funcionamento silencioso","m³/min","5.0"]
["Nível de potência sonora","Arrefecimento","","","dBA","55"]
["","Aquecimento","","","dBA","56"]
["Nível de pressão sonora","Arrefecimento","","Alto","dBA","39"]
["","","","Médio","dBA","33"]
["","","","B","dBA","27"]
["","","","Funcionamento silencioso","dBA","24"]
["","Aquecimento","","Alto","dBA","40"]
["","","","Médio","dBA","33"]
["","","","B","dBA","27"]
["","","","Funcionamento silencioso","dBA","23"]
["Ligações de tubagem","Líquido","","DE","mm","6.35"]
["","Gás","","DE","mm","9.50"]
["","Esgoto","","","","18"]
["Sistemas de controlo","Controlo remoto por infravermelhos","","","","ARC466A2"]
["Acessórios standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Installation plate","","","","1"]
["","Thermal insulation (thermal insulation tube)","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Drain hose","","","","1"]
["","Remote control holder","","","","1"]
["Alimentação elétrica","Nome","","","","V1"]
["","Fase","","","","1~"]
["Alimentação eléctrica","Alimentação eléctrica-=-Frequência","","Frequência","","50"]
["","Alimentação eléctrica-=-Tensão","","Tensão","","220-240"]
["Notas","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]