{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Envolvente","Cor","","","","Branco"]
["Dimensões","Unidade","","Altura","mm","500"]
["","","","Largura","mm","270"]
["","","","Profundidade","mm","270"]
["Peso","Unidade","","","kg","6.8"]
["Operação de purificação do ar","Potência nominal","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","B","kW","0.010"]
["","","","SB","kW","0.008"]
["Nível de pressão sonora","Operação de purificação do ar","","Nível de pressão sonora-=-Operação de purificação do ar-=-Turbo-=-dBA","dBA","53"]
["","","","Médio","dBA","39"]
["","","","B","dBA","29"]
["","","","SB","dBA","19"]
["Ventilador","Caudal de ar","Operação de purificação do ar","Turbo","m³/h","330"]
["","","","Médio","m³/h","192"]
["","","","B","m³/h","120"]
["","","","SB","m³/h","66"]
["Dispositivos de segurança","Item","","01","","Interruptor de segurança (o funcionamento para quando a tampa da unidade Streamer é aberta)"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50/60"]
["","Tensão","","","V CA","220-240/220-230"]
["Corrente de funcionamento","Operação de purificação do ar","","Turbo","A","0.32"]
["","","","Médio","A","0.14"]
["","","","B","A","0.10"]
["","","","SB","A","0.08"]