{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":6,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Envolvente","Cor","","","","Branco"]
["Dimensões","Unidade","","Altura","mm","700 (1)"]
["","","","Largura","mm","270"]
["","","","Profundidade","mm","270 (4)"]
["Peso","Unidade","","","kg","9.5"]
["Operação de purificação do ar","Potência nominal","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","B","kW","0.010"]
["","","","SB","kW","0.007"]
["Operação de humidificação","Potência nominal","","Turbo","kW","0.058"]
["","","","Operação de humidificação-=-Potência nominal-=-M-=-kW","kW","0.019"]
["","","","B","kW","0.014"]
["","","","SB","kW","0.011"]
["","Capacidade do depósito de água","","","l","2.7"]
["Nível de pressão sonora","Operação de purificação do ar","","Nível de pressão sonora-=-Operação de purificação do ar-=-Turbo-=-dBA","dBA","53.0"]
["","","","Médio","dBA","39.0"]
["","","","B","dBA","29.0"]
["","","","SB","dBA","19.0"]
["","Operação de humidificação","","Turbo","dBA","53.0"]
["","","","Médio","dBA","39.0"]
["","","","B","dBA","33.0"]
["","","","SB","dBA","25.0"]
["Ventilador","Caudal de ar","Operação de purificação do ar","Turbo","m³/h","330"]
["","","","Médio","m³/h","192"]
["","","","B","m³/h","120"]
["","","","SB","m³/h","54"]
["","","Operação de humidificação","Turbo","m³/h","330"]
["","","","Médio","m³/h","192"]
["","","","B","m³/h","144"]
["","","","SB","m³/h","102"]
["Acessórios standard","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Alimentação elétrica","Fase","","","","1~"]
["Alimentação eléctrica","Frequência","","","Hz","50/60"]
["","Tensão","","","V CA","220-240/220-230"]
["Corrente de funcionamento","Operação de purificação do ar","","Turbo","A","0.50"]
["","","","Médio","A","0.19"]
["","","","B","A","0.12"]
["","","","SB","A","0.09"]
["","Operação de humidificação","","Turbo","A","0.50"]
["","","","Médio","A","0.20"]
["","","","B","A","0.15"]
["","","","SB","A","0.13"]
["Notas","","","","","(1) - Apenas trifásico"]
["","","","","","(2) - Outra função: Função de reinício automático."]
["","","","","","(3) - Safety valve"]
["","","","","","(4) - Teste a Ta Bs/Bh 14 °C/13 °C. De acordo com EN 16147."]